Reblade and Balance
Most blast wheels come to us in various degree of wear.
When we replace blades, we use an abrasive resistant steel.
Most pneumatic conveyance fans have 1/4-inch blades, but we commonly use ½-inch steel blade replacements.

web builder

After reblading the blastwheel, we use a dynamic balancer
The dynamic balancer can handle up to 2,000lbs with a tip-to-tip of 56 inch diameter.

Outside of these parameters, we would preform a a static balance

Address
111 E. CR 7200
Lubbock, Tx 79464
Contacts
Email: rammfgco@rammfg.net
Phone: +1 (806) 745-5552 Fax: +1 (806)745-5582