Balance and True
Most rotational machinery parts will get out of balance and cause undue wear as well as immediate damage to your equipment.
Usually it is vibration and noise that indicates the need to be balanced.
We can take your blast wheel or cylinder and return it to operational status.
This may require straightening or shaft replacement.

free web templates

After the repair (if any), we use a dynamic balancer
The dynamic balancer can handle up to 2,000lbs with a tip-to-tip of 56 inch diameter.

Outside of these parameters, we would preform a a static balance

Address
111 E. CR 7200
Lubbock, Tx 79464
Contacts
Email: rammfgco@rammfg.net
Phone: +1 (806) 745-5552 Fax: +1 (806)745-5582